For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Disconnect the electrical connector.
3. Remove the motor actuating rod by snapping out it out of the lever with needle-nose pliers.
4. Remove the motor lever.
5. Remove the motor retaining bolts.
6. Remove the mode door motor.

### Installation Procedure

1. Install the mode door motor.
2. Install the motor retaining screws and tighten.
3. Install the motor lever by pressing it onto its shaft.
4. Install the actuating rod.
5. Connect the electrical connector.
6. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .