For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the steering column cover. Refer to Steering Column Trim Covers Replacement .
3. Remove the headlamp switch by pushing in on the tabs on the top and the bottom of the switch housing.
4. Disconnect the electrical connections from the headlamp switch.

### Installation Procedure

1. Connect the electrical connections to the headlamp switch.
2. Install the headlamp switch by snapping it into the switch housing.
3. Install the steering column cover. Refer to Steering Column Trim Covers Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .