For 1990-2009 cars

## Lateral Link Replacement Front

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheels.
3. Remove the rear parallel link bolt-to-knuckle and the bolt-to-rear crossmember.
4. Remove the rear parallel link.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front parallel link bolt-to-knuckle and the cam bolt-to-rear crossmember.

Tighten
Tighten the front parallel link bolt-to-knuckle to 110 N·m (81 lb ft).

2. Adjust the rear toe, if needed. Refer to Rear Toe Adjustment .
3. Tighten the front parallel link cam bolt-to-crossmember.

Tighten
Tighten the cam bolt to 80 N·m (59 lb ft).

## Lateral Link Replacement Rear

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheels.
3. Remove the rear parallel link.
4. Remove the stabilizer shaft-to-stabilizer link nut.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Install the rear parallel link with bolt-to-knuckle and the bolt-to-rear crossmember.

Tighten
Tighten the rear parallel link bolt-to-knuckle and the bolt-to-crossmember to 110 N·m (81 lb ft).