For 1990-2009 cars

## Starter Usage Gasoline Engines

Application | Description
--- | ---
Starter

- No-Load Test @ 12.2 Volts - 2.0L

40-90 A

- No-Load Test Current Draw - 2.0L

1.4 kW

- No-Load Test @ 12.0 Volts - 2.5L

98 A Maximum

- No-Load Test Current Draw - 2.5L

1.7 kW

- Drive Pinion Speed - 2.0L

3,200-4,800 RPM

- Drive Pinion Speed - 2.5L

Minimum 2,600 RPM

Solenoid

- Hold-In Windings @ 12.2 Volts

12-20 A

- Pull-In Windings @ 12.2 Volts

60-90 A

## Starter Usage Diesel Engine

Description | Specification
--- | ---
Unit | Standard
Type | -- | PG 260NS
Capacity | Kw | 1.55
No Load Test at 12 volts Condition Drive Pinion Speed | A | 95 MAX
Pinion Gear Speed | RPM | 2 550 MIN (@12V)