For 1990-2009 cars

## Battery Usage Gasoline Engines

Application | Description
--- | ---
Cold Cranking Amperage - 2.0L | 550 A (cold area: 610 A)
Cold Cranking Amperage - 2.5L | 610 A
Reserve Capacity Minimum - 2.0L | 90 minutes
Reserve Capacity Minimum - 2.5L | 110 minutes
Load Test | 270 A
Minimum Voltage: | Estimated Temperature:

- 9.6

- 21°C (69.8°F)

- 9.4

- 20°C (68°F)

- 9.1

- 0°C (32°F)

- 8.8

- -10°F (14°F)

- 8.5

- -18°C (0°F)

- 8.0

Below -18°C (Below 0°F)

## Battery Usage Diesel Engine

Description | Specification
--- | ---
Unit | Standard
Type | -- | Maintenance Free
Output (Capacity) | V-AH | 12V-90AH
Cold Cranking Amps (CCA) | CCA | 610
Load Test | amps | 305
Minimum Voltage

- 9.6

V

21°C (70°F) and above

- 9.5

V

15.6°C (60°F)

- 9.4

V

10°C (50°F)

- 9.3

V

4.4°C (40°F)

- 9.1

V

-1.1°C (30°F)

- 8.9

V

-6.7°C (20°F)

- 8.7

V

-12.2°C (10°F)

- 8.5

V

-17.8°C (0°F)