For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the right front wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the front wheel well splash shield. Refer to Wheelhouse Splash Shield Replacement.
4. Disconnect the electrical connector.
5. Disconnect the washer hose from the washer pump.
6. Remove the washer pump.

### Installation Procedure

1. Install the washer pump.
2. Connect the washer hose to the washer pump.
3. Connect the electrical connector.
4. Install the front wheel well splash shield. Refer to Wheelhouse Splash Shield Replacement.
5. Install the right front wheel. Refer to Tire and Wheel Removal and Installation .
6. Connect the negative battery cable.