For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster. Refer to Instrument Cluster Replacement .
3. Press the clips down and remove the instrument cluster lens.
4. Remove the screws and the instrument cluster case.
5. Remove the screws and the speedometer from the instrument cluster.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the speedometer with the screws.

Tighten
Tighten the speedometer screws to 2 N·m (18 lb in).

2. Install the instrument cluster case with the screws.
3. Install the instrument cluster lens.
4. Install the instrument cluster. Refer to Instrument Cluster Replacement .
5. Connect the negative battery cable.