For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Release the connector lock and pull the transducer wire connector out.
3. Remove the transducer with a wrench.
4. Discard the O-ring seal.

### Installation Procedure

1. Install the new O-ring seal on the transducer.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the pressure transducer.

Tighten
Tighten the pressure transducer to 7 N·m (62 lb in).

3. Connect the wire connector.
4. Connect the negative battery cable.