For 1990-2009 cars

Warning: The transaxle fluid is hot. Caution must be taken to prevent personal injury when the transaxle fluid drains from the transaxle.

1. Raise and support the vehicle.
2. Remove the transaxle drain plug and allow the transaxle to drain completely.
3. Remove the fluid level check plug.

Caution: Refer to Fastener Caution in the Preface section.

4. Clean and install the transaxle drain plug and tighten to 6 N·m (53 lb in) plus an additional 45-180 degrees.
5. Add SAE75W90 transaxle fluid until it seeps out of the fluid level check plug.
6. Clean and install the fluid level check plug and tighten to 6 N·m (53 lb in) plus an additional 45-180 degrees.
7. Lower the vehicle and verify proper operation.

Fluid Specification | SAE75W90
--- | ---
Fluid Capacity | FWD | 2.1L (2.22 qt)