For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Open the glove box.
3. Remove the glove box lamp.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the glove box lamp.
3. Close the glove box.
4. Connect the negative battery cable.