For 1990-2009 cars

Checks | Causes
--- | ---
Differential Assembly (232) |

• | Inspect for worn or damaged Side Gear Thrust Washer or Pinion Gear Thrust Washer.

• | Inspect for loose or worn Side Gear Axle Splines.

• | Inspect for damaged or worn Side Gear.

• | Inspect for worn or damaged Final Drive Inner and Outer Washers (584).

• | Inspect for loose, damaged or worn Front Differential Carrier Thrust Bearings, (228, 231, 233).

• | Inspect for broken, worn or disengaged Final Drive Pinion Pin Retainer (581).

• | Inspect for damaged or worn Pinion Gears.

Drive Link Assembly (225) |

• | Inspect for worn, loose or damaged links.

• | Inspect for broken, worn or loose Drive Link Lube Scoop (60).

Drive Sprocket Assembly (224) |

• | Inspect for improper Drive Sprocket (224) tooth surface finish.

• | Inspect for broken or damaged Drive Sprocket (224) teeth.

• | Inspect for worn or damaged Drive Sprocket Thrust Bearings (223, 556).

• | Inspect for worn or damaged Output Carrier Transfer Drive Gear Hub Assembly splines (222).

• | Inspect for loose, worn or damaged Output Carrier Transfer Drive Gear Hub Assembly bushing.

Driven Sprocket Assembly (229) |

• | Inspect for worn, binding or damaged Driven Sprocket Bearing Assembly (228).

• | Inspect for worn or damaged Driven Sprocket Ball Bearing Assembly.

• | Inspect for improper Driven Sprocket (229) tooth surface finish.

• | Inspect for broken or damaged Driven Sprocket (229) teeth.

Input Carrier Assembly (570) |

• | Inspect for pitted/spalled Pinion Gear teeth.

• | Inspect for worn or damaged Pinion Gear Thrust Washers and Bushings.

• | Inspect for worn or damaged Pinion Gears, Pins or Needle Bearings.

• | Inspect for loose or broken Hub and Ring Gear.

• | Inspect for loose or broken Output Internal Gear Retainer.

• | Inspect for loose or worn Sun Gear Thrust Bearings (569, 572).

Output Carrier Assembly (574) |

• | Inspect for worn or damaged Pinion Gear Thrust Washers and Bushings.

• | Inspect for worn or damaged Pinion Gears, Pins or Needle Bearings.

• | Inspect for loose Hub and Ring Gear.

Output Sun Gear Assembly (555) |

• | Inspect for worn or damaged Output Sun Gear Thrust Bearing (556).

• | Inspect for loose, worn or damaged Output Sun Gear bushing.

• | Inspect for worn or damaged Output Sun Gear teeth.

Reaction Carrier Assembly (567) |

• | Inspect for worn or damaged Pinion Gear Thrust Washers and Bushings.

• | Inspect for worn or damaged Pinion Gears, Pins or Needle Bearings.

• | Inspect for loose hub and Ring Gear.

• | Inspect for worn or damaged Reaction Carrier Thrust Bearings (565).

Reaction Sun Gear Assembly (566) | Inspect for loose, worn or damaged Reaction Sun Gear Assembly bushing.
Fluid Pump Assembly (201) |

1. Inspect for proper fluid level.
2. Inspect for leaking Pump Fluid Outlet Seal Assembly (24) or Filter Seal.

3-5-Reverse Clutch Assembly |

• | Inspect for inadequate Clutch Plate Clearance.

• | Inspect for stripped or sheared Clutch Plate Splines (508-510).

• | Inspect for loose or worn Backing Plate Retainer (511).

• | Inspect for loose Speed Sensor Reluctor Wheel (501) or Retainer (500).

4-5-6 Clutch Assembly |

• | Inspect for inadequate Clutch Plate Clearance.

• | Inspect for stripped or sheared Clutch Plate Splines (425-428).

• | Inspect for loose or worn Clutch Dam Retainer (524).

• | Inspect for loose or worn 3-5-Reverse/4-5-6 Clutch Housing Bushing.

1-2-3-4 Clutch Assembly |

• | Inspect for inadequate Clutch Plate Clearance.

• | Inspect for stripped or sheared Clutch Plate Splines (557-559).

• | Inspect for loose or worn Clutch Spring Retainer (561).

Low and Reverse Clutch Assembly (OWC) (543) |

• | Inspect for stripped or sheared Low and Reverse Clutch Assembly (543) splines.

• | Inspect for non-rotating Low and Reverse Clutch Assembly (543).

Low and Reverse Clutch |

• | Inspect for inadequate Clutch Plate Clearance.

• | Inspect for stripped or sheared Clutch Plate Splines (545-547).

• | Inspect for loose or worn Clutch Spring Retainer (548).

2-6 Clutch Assembly |

• | Inspect for inadequate Clutch Plate Clearance.

• | Inspect for stripped or sheared Clutch Plate Splines (540-542).

• | Inspect for loose or worn Clutch Spring Retainer (537).

Case Assembly (50) |

• | Inspect for loose or broken Transmission Mount Bolts.

• | Inspect for loose Torque Converter and Differential Housing Bolts (26).

• | Inspect for loose, worn or damaged differential bushing.

• | Inspect for loose or broken Input Shaft Support Bolts (57).

• | Inspect for loose or broken Front Differential Carrier Baffle Bolts (61).

• | Inspect for stripped or sheared splines.

• | Inspect for loose, worn or damaged bushing.

Torque Converter Housing Assembly (208) |

• | Inspect for loose or broken Front Differential Ring Gear Retainer (206).

• | Inspect for loose, worn or damaged differential bushing.

• | Inspect for loose or broken Pinion Gear Shaft Retainer Pin.

• | Inspect for loose or broken Front Differential Carrier Baffle Bolts (204).

• | Inspect for loose or broken Fluid Pump Bolts (200).

• | Inspect for loose Torque Converter and Differential Housing Bolts (26).

• | Inspect for loose, worn or damaged bushing.

Control Valve Body Cover Assembly (2) | Inspect for loose, missing or broken Valve Body Cover Bolts (1).
Torque Converter (28) |

• | Inspect for improper alignment of Torque Converter to the Crankshaft.

• | Inspect for ballooning of the Torque Converter.

Differential Carrier Assembly (232) |

• | Inspect for worn or damaged Differential Carrier (582).

• | Inspect for worn or damaged Pinion Pins (583).

• | Inspect for broken, worn or damaged Differential Sun Gear Bearing (231) or Driven Sprocket Bearing (228).

• | Inspect for worn or damaged Differential Side Gear teeth, Final Drive Pinion Gear (586) teeth or Final Drive Sun Gear (230) teeth.

• | Inspect for worn or damaged Differential Side Gear Thrust Washers or Final Drive Inner and Outer Washers (584).

• | Inspect for worn or damaged Final Drive Rollers (585).

• | Inspect for broken or damaged Differential Pinion Gear Shaft Retainer.