For 1990-2009 cars

1. Remove the engine undercover shield. Refer to Engine Shield Replacement.
2. Drain the engine oil.
3. Remove the oil pan. Refer to Oil Pan Replacement.
4. Remove the oil strainer with washer.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the oil strainer with washer.

• | Tighten the oil strainer bolt to 11 N·m (97.4 lb in).

• | Tighten the oil strainer bracket bolt (bed plate outer bolt) to 35 N·m (25.8 lb ft).

2. Install the oil pan. Refer to Oil Pan Replacement.
3. Fill the engine with engine oil.
4. Install the engine undercover shield. Refer to Engine Shield Replacement.