For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the glove box lower panel cover. Refer to Instrument Panel Storage Compartment Replacement.
3. Disconnect the electrical connector.
4. Remove the actuating rod by snapping it out of the lever with needle-nose pliers.
5. Remove the motor lever from its shaft by pulling the lever off.
6. Remove the motor retaining screws.
7. Remove the temperature door motor.

### Installation Procedure

1. Install the temperature door motor.
2. Install the retaining screws and tighten.
3. Press the lever onto motor shaft.
4. Install the actuating rod onto the lever.
5. Connect the electrical connector.
6. Install the glove box lower panel cover. Refer to Instrument Panel Storage Compartment Replacement.
7. Connect the negative battery cable.