For 1990-2009 cars

#### Special Tools

DT-47599 Anchor Bolt Socket

1. Install the third gear band assembly (16) into the transmission case assembly making sure that the band tangs are located at the servo pin and the 3rd gear band anchor bolt hole (64).
2. Inspect the anchor bolt and the bolt hole.
3. Apply automatic transmission fluid to a new O-ring (65).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the new O-ring and third gear band anchor bolt (64) using DT-47599 and tighten to 167 N·m (123 lb ft).