For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.
2. Remove the screws and the instrument cluster.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the instrument cluster with the screws and tighten to 2 N·m (18 lb in).
2. Install the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.