For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front door step lamp lens cover.
3. Reposition the lower half of the front door trim panel.
4. Remove the front door step lamp.
5. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the replacement front door step lamp bulb.
3. Install the lower half of the door trim panel to its original position.
4. Install the front door step lamp lens cover.
5. Connect the negative battery cable.