For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Pry off the vanity mirror lamp lens by inserting a screwdriver into the recess along the bottom edge of the lens.
3. Remove the inoperative bulb.

### Installation Procedure

1. Install the replacement bulb.
2. Press the vanity mirror lamp lens onto the housing.
3. Connect the negative battery cable.