For 1990-2009 cars

### Removal Procedure

1. Remove the caliper. Refer to Rear Brake Caliper Replacement .
2. Remove the brake shoes.
3. Remove the caliper mounting bracket.
4. Remove the rotor detent screw.
5. Remove the rotor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: To guarantee uniform braking, always refinish both rotors even if only one rotor is defective.

1. Install the rotor on the hub and install the detent screw.

Tighten
Tighten the rotor detent screw to 4 N·m (35 lb in).

2. Apply a few drops of thread-locking compound to the caliper bracket mounting bolts and install the caliper bracket.

Tighten
Tighten the caliper bracket mounting bolts to 45 N·m (33 lb ft).

3. Install the brake shoes and the caliper. Refer to Rear Brake Caliper Replacement .