For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the stoplamp switch electrical connector.
3. Twist the switch, and remove the switch from the brake pedal bracket.

### Installation Procedure

1. Adjust the stoplamp switch. Refer to Stop Lamp Switch Adjustment.
2. Connect the negative battery cable.