For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Disconnect the windshield washer hose from the washer nozzles on the hood.
3. Remove the front right wheel. Refer to Tire and Wheel Removal and Installation.
4. Remove the front wheel well splash shield. Refer to Wheelhouse Splash Shield Replacement.
5. Disconnect the washer hose from the washer reservoir.
6. Remove the washer hose.

### Installation Procedure

1. Connect the washer hose to the washer pump.
2. Install the front wheel well splash shield. Refer to Wheelhouse Splash Shield Replacement.
3. Install the front right wheel. Refer to Tire and Wheel Removal and Installation.
4. Connect the windshield washer hose to the washer nozzles on the hood.
5. Close the hood.