For 1990-2009 cars

1. Move the shift control lever into the N - Neutral position.

Important: The shift control cable must be disconnected from the transmission range selector lever prior to disconnecting it from the control cable bracket. Otherwise, damage to the manual shift shaft may result, requiring transaxle disassembly.

2. Disconnect the shift control cable from the TR selector lever.
3. Disconnect the shift control cable from the control cable bracket by depressing the control cable retainer clip tabs and pulling up. Discard the clip.
4. Release the shift control cable assembly adjustment lock.
5. Slide the black tab back.
6. Insert a screwdriver into the slot under the white tab and pull up on the white tab.
7. Install the shift control cable into the shift control cable bracket. Secure with a new shift control cable retainer clip. An audible snap will be heard when properly installed.
8. With the selector lever in neutral (N), snap the cable end fitting onto the ball stud of the switch lever. An audible snap will be heard when properly installed.
9. Lock the control cable adjustment tab.
10. Push down on the white tab to secure.
11. Slide the black tab over the white tab to lock in place.
12. Verify the proper operation.