For 1990-2009 cars

## Clutch Grabbing D33 Manual Transaxle

Checks | Actions
--- | ---
Check for a contaminated or warped flywheel. | Repair or replace the flywheel.
Check for a weak diaphragm spring. | Replace the necessary clutch components. Refer to Clutch Assembly Replacement .
Check for a oily contamination of the clutch disc. | Replace the necessary clutch components.
Check for worn splines on the input shaft. | Replace the splines on the input shaft.

## Clutch Grabbing D24 Manual Transaxle

Checks | Actions
--- | ---
Check for a burned or a glazed facing caused by oil on the facing. | Correct the leak at its source and install anew clutch disc.
Check for worn splines on the input shaft. | Replace the worn input shaft.
Check for a warped pressure plate or a warped flywheel. | Replace the warped pressure plate or the warped flywheel.
Check for burned or smeared resin on the flywheel or the pressure plate. | Sand off the burned or smeared resin if it is superficial. Replace any burned or heat-checked parts.