For 1990-2009 cars

### Throttle Positions

Engine Braking: A condition where the engine is used to slow the vehicle by manually downshifting during a zero throttle coastdown.
Full Throttle Detent Downshift: A quick apply of the accelerator pedal to its full travel, forcing a downshift.
Heavy Throttle: Approximately 3/4 of accelerator pedal travel, 75 percent throttle position.
Light Throttle: Approximately 1/4 of accelerator pedal travel, 25 percent throttle position.
Medium Throttle: Approximately 1/2 of accelerator pedal travel, 50 percent throttle position.
Minimum Throttle: The least amount of throttle opening required for an upshift.
Wide Open Throttle (WOT): Full travel of the accelerator pedal, 100 percent throttle position.
Zero Throttle Coastdown: A full release of the accelerator pedal while the vehicle is in motion and in drive range.

### Shift Condition Definitions

Bump: A sudden and forceful apply of a clutch or a band.
Chuggle: A bucking or jerking. This condition may be most noticeable when the converter clutch is engaged. It is similar to the feel of towing a trailer.
Delayed: A condition where a shift is expected but does not occur for a period of time. This could be described as a clutch or band engagement that does not occur as quickly as expected during a part throttle or wide open throttle apply of the accelerator, or during manual downshifting to a lower range. This term is also defined as LATE or EXTENDED.
Double Bump - Double Feel: Two sudden and forceful applies of a clutch or a band.
Early: A condition where the shift occurs before the car has reached proper speed. This condition tends to labor the engine after the upshift.
End Bump: A firmer feel at the end of a shift than at the start of the shift. This is also defined as END FEEL or SLIP BUMP.
Firm: A noticeably quick apply of a clutch or band that is considered normal with a medium to heavy throttle. This apply should not be confused with HARSH or ROUGH.
Flare: A quick increase in engine RPM along with a momentary loss of torque. This most generally occurs during a shift. This condition is also defined as SLIPPING.
Harsh - Rough: A more noticeable apply of a clutch or band than FIRM. This condition is considered undesirable at any throttle position.
Hunting: A repeating quick series of upshifts and downshifts that causes a noticeable change in engine RPM, such as a 4-3-4 shift pattern. This condition is also defined as BUSYNESS.
Initial Feel: A distinctly firmer feel at the start of a shift than at the finish of the shift.
Late: A shift that occurs when the engine RPM is higher than normal for a given amount of throttle.
Shudder: A repeating jerking condition similar to CHUGGLE but more severe and rapid. This condition may be most noticeable during certain ranges of vehicle speed.
Slipping: A noticeable increase in engine RPM without a vehicle speed increase. A slip usually occurs during or after initial clutch or band apply.
Soft: A slow, almost unnoticeable clutch or band apply with very little shift feel.
Surge: A repeating engine related condition of acceleration and deceleration that is less intense than CHUGGLE.
Tie-Up: A condition where two opposing clutch and/or bands are attempting to apply at the same time causing the engine to labor with a noticeable loss of engine RPM.

### Noise Conditions

Drive Link Noise: A whine or growl that increases or fades with vehicle speed, and is most noticeable under a light throttle acceleration. It may also be noticeable in PARK or NEUTRAL operating ranges with the vehicle stationary.
Final Drive Noise: A hum related to vehicle speed which is most noticeable under a light throttle acceleration.
Planetary Gear Noise: A whine related to vehicle speed, which is most noticeable in FIRST gear, SECOND gear, FOURTH gear or REVERSE. The condition may become less noticeable, or go away, after an upshift.
Pump Noise: A high pitched whine that increases in intensity with engine RPM. This condition may also be noticeable in all operating ranges with the vehicle stationary or moving.
Torque Converter Noise: A whine usually noticed when a vehicle is stopped, and the transmission is in DRIVE or REVERSE. The noise will increase with engine RPM.

### Transmission Abbreviations

A/C: Air Conditioning
AC: Alternating Current
AT: Automatic Transmission
CAN: Controller Area Network
CCDIC: Climate Control Driver Information Center
DC: Direct Current
DIC: Driver Information Center
DLC: Diagnostic Link Connector
DMM: Digital Multimeter
DTC: Diagnostic Trouble Code
EBTCM: Electronic Brake/Traction Control Module
ECCC: Electronically-Controlled Capacity Clutch
ECT: Engine Coolant Temperature
EMI: Electromagnetic Interference
IAT: Intake Air Temperature
IGN: Ignition
IMS: Internal Mode Switch
ISS: Input Speed Sensor
MAP: Manifold Absolute Pressure
MIL: Malfunction Indicator Lamp
NC: Normally Closed
NO: Normally Open
OBD: On Board Diagnostic
OSS: Output Speed Sensor
PC: Pressure Control
PCM: Powertrain Control Module
PWM: Pulse Width Modulation
RPM: Revolutions Per Minute
SS: Shift Solenoid
STL: Service Transmission Lamp
TAP: Transmission Adaptive Pressure
TCC: Torque Converter Clutch
TCM: Transmission Control Module
TFP: Transmission Fluid Pressure
TFT: Transmission Fluid Temperature
TP: Throttle Position
TR: Transaxle Range
TV: Throttle Valve
VCM: Vehicle Control Module
VSS: Vehicle Speed Sensor
WOT: Wide Open Throttle