For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear wheels.
3. Remove the rear brake caliper and remove the rear disc brake and screw.
4. Remove the rear hub nuts-to-knuckle and the rear hub.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear hub nuts-to-knuckle and tighten to 65 N·m (48 lb ft).
2. Install the rear disc brake and the rear brake caliper and tighten to 45 N·m (33 lb ft).
3. Install the rear brake disc screw and tighten to 4 N·m (35 lb in).