For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Important: Only lift the engine far enough to take the weight off the transaxle rear mount assembly, or damage to the mount and lifting equipment failure may occur.

1. Support the engine assembly using DW-110-060 .
2. Remove the engine shield. Refer to Engine Shield Replacement .
3. Remove the front crossmember. Refer to Engine Front Crossmember Replacement .
4. Remove the engine rear mount from the transaxle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the engine rear mount to the transmission.

Tighten
Tighten the engine rear mount retaining bolts to 90 N·m (66 lb ft).

2. Install the front crossmember. Refer to Engine Front Crossmember Replacement .
3. Install the engine shield. Refer to Engine Shield Replacement .
4. Remove the engine support fixture DW-110-060 .