For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the console. Refer to Front Floor Console Replacement .
3. Disconnect the shift control cables from the shift control lever housing. Refer to Shift Control Linkage Replacement .
4. Remove the nuts and bolts from the shift control lever housing.
5. Remove the shift control lever housing.

### Installation Procedure

1. Install the shift control lever housing.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts and bolts to the shift control lever housing.

Tighten
Tighten the shift control lever housing bolts to 8 N·m (71 lb in).

3. Connect the shift control cables to the shift control lever housing, and adjust the cable. Refer to Shift Control Linkage Replacement .
4. Install the console. Refer to Front Floor Console Replacement .
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .