For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the screws and the instrument cluster.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the instrument cluster with the screws.

Tighten
Tighten the instrument cluster screws to 2 N·m (18 lb in).

2. Install the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .