For 1990-2009 cars

Checks | Actions
--- | ---
Check for the driver improperly operating the vehicle. | Correct the driver's operation of the vehicle, as necessary.
Check for a binding release bearing. | Clean and re-lubricate the release bearing. Inspect the release bearing for burrs and nicks.
Check for an improperly installed release lever. | Remove and reinstall the release lever properly.
Check for a weak linkage return spring. | Replace the weak linkage return spring.