For 1990-2009 cars

## Clutch Slipping D33 Manual Transaxle

Checks | Actions
--- | ---
Check for a stuck concentric slave cylinder. | Replace the concentric slave cylinder. Refer to Clutch Concentric Actuator Cylinder Replacement.
Check for improper return of clutch oil. | Perform the air bleeding.
Check for a worn clutch disc or oil contamination. | Replace the necessary clutch components. Refer to Clutch Assembly Replacement.
Check for a warped pressure plate. | Replace the necessary clutch components.

## Clutch Slipping D24 Manual Transaxle

Checks | Actions
--- | ---
Check for the driver improperly operating the vehicle. | Correct the driver's operation of the vehicle, as necessary.
Check for an oil-soaked clutch disc. | Correct the leak at its source and install a new clutch disc.
Check for a worn facing or a facing torn from the disc. | Replace the worn disc with a new disc.
Check for a warped pressure plate or a warped flywheel. | Replace the warped pressure plate or the warped flywheel.
Check for a weak diaphragm spring. | Replace the pressure plate.