For 1990-2009 cars

### Removal Procedure

1. Remove the door trim. Refer to Front Side Door Trim Panel Replacement .
2. Slide the door handle rearward and remove it from the door.
3. Disconnect the inside door handle and the lock rods.

### Installation Procedure

1. Connect the inside door handle and the lock rods.
2. Insert the inside door handle into the slots in the door.
3. Slide the door handle forward.
4. Install the door seal trim. Refer to Front Side Door Trim Panel Replacement .