For 1990-2009 cars

Application | Trim Height
--- | ---
195/70R14 | 205/65R15 | 205/55R16
Bottom of Front Wheel to Bottom of Front Wheel Well | 676 ± 15 mm (26.6 in) | 685 ± 15 mm (27 in) | 676 ± 15 mm (26.6 in)
Bottom of Rear Wheel to Bottom of Rear Wheel Well | 678 ± 15 mm (26.7 in) | 686 ±15 mm (27 in) | 678 ± 15 mm (26.7 in)
Note: The above specifications are with the vehicle in a normally loaded condition. Prior to inspecting the vehicle, place a weight of approximately 68 kg (150 lb) on each front seat cushion.