For 1990-2009 cars

### Removal Procedure

1. Remove the screws that hold the trim panel to the instrument panel.
2. Remove the trim panel.
3. Remove the driver side knee bolster. Refer to Knee Bolster Replacement.
4. Remove the stop lamp switch. Refer to Stop Lamp Switch Replacement.
5. Disconnect the spring retaining clip and the bolt from the pushrod clevis.
6. Remove the hex nut and the spring.
7. Remove the brake pedal and the bolt.
8. Remove the brake pedal cover. Manual transaxle pedal shown

### Installation Procedure

1. Install a new pedal cover, if needed. Automatic transaxle pedal shown
2. Coat the pedal shaft with grease.
3. Position the brake pedal on the pedal-to-dash panel bracket and the pedal bolt.

Caution: Refer to Fastener Caution in the Preface section.

4. Place the hex nut and the spring on the pedal bolt and tighten to 18 N·m (13 lb ft).
5. Install the pushrod clevis to the pedal with the bolt and the spring retaining clip.
6. Connect the stop lamp switch and connector assembly to the pedal bracket. Refer to Stop Lamp Switch Replacement.
7. Install the knee bolster. Refer to Knee Bolster Replacement.
8. Install the trim panel with the screws and tighten to 3 N·m (27 lb in).