For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Disconnect the brake line from the disc brake hose at the wheel housing bracket on each side of the vehicle.
3. Remove the brake hose retainer.
4. Remove the rear disc brake hose retainer and the brake hose from the bracket on the steering knuckle shaft.
5. Remove the rear disc brake hose from the caliper.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear disc brake hose to the caliper.

Tighten
Tighten the rear disc brake hose-to-caliper bolt to 32 N·m (24 lb ft).

2. Install the rear disc brake hose and the retainer on the bracket on the steering knuckle shaft.
3. Install the rear disc brake line to the brake hose on the wheel housing bracket.

Tighten
Tighten the brake line to fittings to 16 N·m (12 lb ft).

4. Lower the vehicle.
5. Bleed the brake system. Refer to Hydraulic Brake System Bleeding .
6. Check the brake system for leaks.