For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement.
3. Remove the screw and the guide rail.
4. Remove the door lock screws.
5. Disconnect the lock rods.
6. Remove the door lock.
7. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the rear door lock with the screws and tighten to 10 N·m (89 lb in).
3. Install the lock rods.
4. Install the guide rail with the bolts and the screw. Tighten the screw to 4 N·m (35 lb in) and the bolts to 10 N·m (89 lb in).
5. Install the door seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement.
6. Connect the negative battery cable.