For 1990-2009 cars

### Removal Installation

1. Press in the head restraint adjust button and remove the head restraint from the seat back.
2. Insert 2 flat-head screwdrivers down the front and back side of the guide sleeves.
3. With the screwdrivers, press in the retaining latches and remove the guide sleeves.

### Installation Procedures

1. Install the guide sleeves into the seat back and press them down to engage the guide sleeve retaining latches.
2. Install the head restraint into the guide sleeves.