For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Module Retaining Bolt | 9 N·m | 79.7 lb in
Beauty Cover Bracket Bolt | 11 N·m | 97.4 lb in
Boost Pressure Sensor (T-Map Sensor) Bolt | 8 N·m | 70.8 lb in
CKP Sensor Retaining Bolt | 7 N·m | 62 lb in
CMK Sensor Retaining Bolt | 7 N·m | 62 lb in
Common Rail Pressure Sensor | 70 N·m | 51.6 lb ft
Common Rail Regulator | 85 N·m + 60-90° | 62.7 lb ft + 44.3-90°
Common Rail Retaining Bolt | 25 N·m | 18.4 lb ft
DPF Pressure Sensor Bracket Bolt | 10 N·m | 88.5 lb in
DPF Pressure Sensor Pipe Retaining Nut | 4 N·m | 35.4 lb in
DPF Retaining Nut | 30 N·m | 22.1 lb ft
ECM Bracket Retaining Nut | 15 N·m | 11.1 lb ft
ECT Sensor | 35 N·m | 25.8 lb ft
EGR Cooler Inlet Pipe Retaining Nut (to EGR Valve) | 20 N·m | 14.8 lb ft
EGR Cooler Inlet Pipe Retaining Nut (to Exhaust Manifold) | 33 N·m | 24.3 lb ft
EGR Cooler Outlet Pipe Retaining Bolt and Nut | 20 N·m | 14.8 lb ft
EGR Cooler Retaining Nut (Engine Wiring Harness Bracket Nut) | 20 N·m | 14.8 lb ft
EGR Vacuum Solenoid Valve Retaining Bolt | 7 N·m | 62 lb in
EGR Valve Retaining Bolt (to EGR Inlet Pipe) | 20 N·m | 14.8 lb ft
EGR Retaining Nut (to EGR Cooler) | 20 N·m | 14.8 lb ft
ETC Retaining Bolt and Nut | 9 N·m | 79.7 lb in
Exhaust Gas Temperature Sensor 1 | 45 N·m | 33.2 lb ft
Exhaust Gas Temperature Sensor 2 | 45 N·m | 33.2 lb ft
Fuel Filter Bracket Nut | 10 N·m | 88.5 lb in
Fuel Filter Locker | 30 N·m | 22.1 lb ft
Fuel Pipe-to-Common Rail Nut (M14) (M17) | 20 N·m | 14.8 lb ft
Fuel Pipe-to-Common Rail Retaining Bolt | 10 N·m | 88.5 lb in
Fuel Pipe-to-Injection Pump Retaining Bolt (to Cylinder Head Cover) | 25 N·m | 18.4 lb ft
Fuel Pipe-to-Injection Pump Retaining Bolt (to Intake Manifold) | 9 N·m | 79.7 lb in
Fuel Pipe-to-Injector Nut (M14) | 27 N·m | 19.9 lb ft
Fuel Pipe-to-Injector Nut (M17) | 20 N·m | 14.8 lb ft
Fuel Tank Strap Retaining Nut | 20 N·m | 14.8 lb ft
Function Block Retaining Bolt | 11 N·m | 97.4 lb in
Glow Plug | 9 N·m | 79.7 lb in
Glow Plug Fuse Box Retaining Bolt | 10 N·m | 88.5 lb in
Glow Plug Heat Shield Bolt | 20 N·m | 14.8 lb ft
Glow Plug Heat Shield Nut (Engine Lift Bracket Retaining Nut) | 28 N·m | 20.6 lb ft
Glow Plug Module Retaining Nut | 14 N·m | 10.3 lb ft
Injection Pump Sprocket Nut | 70 N·m | 51.6 lb ft
Injection Pump Tightening Bolt | 30 N·m | 22.1 lb ft
Injector Bracket Bolt | 28 N·m | 20.7 lb ft
Injector Bracket Plug Bolt | 7 N·m | 62 lb in
Oil Pressure Switch | 30 N·m | 22.1 lb ft
Turbocharger Tightening Nut | 34 N·m | 25.1 lb ft
Turbocharger Wheel Bearing Oil Inlet Pipe Bolt | 23 N·m | 17 lb ft
Turbocharger Wheel Bearing Oil Outlet Pipe Bolt | 12 N·m | 8.9 lb ft
Vacuum Pump Tightening Bolt | 12 N·m | 8.9 lb ft
Water Pipe Retaining Bolt (M6) | 9 N·m | 79.7 lb in
Water Pipe Retaining Bolt (M8) | 20 N·m | 14.8 lb ft