For 1990-2009 cars

### Removal Procedure

Note: Install protective coverings over the fenders and the windshield to prevent damage to the paint, the glass, and the moldings when removing and installing the hood.

1. Raise and support the hood.
2. Mark the position of the hinge to the hood to aid in alignment during installation.
3. Remove the washer hoses from the hood.
4. Remove the hood struts. Refer to Hood Hold-Open Rod Replacement.
5. Remove the bolts retaining the hood to both of the hinges.
6. With the aid of another technician, remove the hood from the hinges.

### Installation Procedure

1. With the aid of another technician, position the hood in the location marked during removal.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 2 bolts securing the hood to each hinge and tighten to 24 N·m (18 lb ft).
3. Install the hood struts. Refer to Hood Hold-Open Rod Replacement.
4. Inspect the hood for proper alignment.
5. Install the washer hoses to the hood.