For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the crankshaft position (CKP) sensor connector.
3. Remove the CKP sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the CKP sensor.

Tighten
Tighten the CKP sensor retaining bolt to 7 N·m (62 lb in).

2. Connect the CKP sensor.
3. Connect the negative battery cable.