For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the bolts and the headlamp assembly.
3. Disconnect the headlamp assembly electrical connectors.
4. Remove the cap that conceals the headlamp bulb.
5. Disconnect the headlamp bulb electrical connectors.
6. Remove the headlamp bulbs.

### Installation Procedure

Caution: Refer to Halogen Bulb Caution in the Preface section.

1. Install the headlamp bulbs.
2. Connect the headlamp bulb electrical connectors.
3. Install the cap that conceals the headlamp bulbs.
4. Connect the headlamp assembly electrical connectors.
5. Install the headlamp assembly with the bolts.
6. Connect the negative battery cable.