For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Separate the plastic clip from the end of each ball socket.
3. Separate the ball sockets from the ball studs on the linkage bolts using a pry bar.
4. Remove the control shift rod from the vehicle.

### Installation Procedure

1. Install the control shift rod into the vehicle.
2. Press the ball sockets onto the ball studs on the linkage bolts.
3. Connect the plastic clip on the end of each ball socket.
4. Connect the negative battery cable.