For 1990-2009 cars

### Removal Procedure

1. Raise the hood.
2. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement.
3. Remove the weatherstrip.
4. Remove the air inlet grille retaining screws, clips, and the 2-piece grille.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the 2-piece grille with the air inlet grille retaining clips and screws and tighten to 3 N·m (27 lb in).
2. Install the weatherstrip.
3. Install the wiper arms. Refer to Windshield Wiper Arm Replacement.
4. Lower the hood.