For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheels.
3. Remove the trailing link bolt-to-knuckle and the trailing link bracket bolts.
4. Remove the trailing link.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Install the trailing link with bolt-to-knuckle and the bolts-to-trailing link bracket.

Tighten

• | Tighten the trailing link bolt-to-knuckle to 120 N·m (89 lb ft).

• | Tighten the trailing link bracket bolts to 90 N·m (66 lb ft).