For 1990-2009 cars

### Removal Procedure

Important: Left-Hand Drive Shown, Right-Hand Drive Similar.

1. Open the hood.
2. Remove the nut from the wiper arm.
3. Pull the wiper arm off.

### Installation Procedure

1. Install the wiper arm.

Notice: Refer to Fastener Notice in the Preface section.

2. Secure the wiper arm with the nut.

Tighten
Tighten the wiper arm nut to 22 N·m (16 lb ft).

3. Close the hood.