For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the I/P storage compartment. Refer to Instrument Panel Storage Compartment Replacement.
3. Remove the actuating rod by snapping the rod out of the lever with needle-nose pliers.
4. Remove the actuating lever.
5. Disconnect the electrical connector.
6. Remove the motor retaining screws.
7. Remove the motor.

### Installation Procedure

1. Install the motor.
2. Install the motor retaining bolts and tighten.
3. Install the actuating lever.
4. Install the actuating rod.
5. Connect the electrical connector.
6. Remove the I/P storage compartment. Refer to Instrument Panel Storage Compartment Replacement.
7. Connect the negative battery cable.