For 1990-2009 cars

## Fastener Tightening Specifications Gasoline

Application | Specification
--- | ---
Metric | English
Catalytic Converter-to-Connecting Pipe Nuts | 40 N·m | 30 lb ft
Catalytic Converter-to-Exhaust Manifold Nuts | 40 N·m | 30 lb ft
Connecting Pipe Mounting Bracket Nuts | 30 N·m | 22 lb ft
Exhaust Front Muffler-to-Exhaust Front Pipe Nuts | 40 N·m | 30 lb ft
Exhaust Front Pipe-to-Exhaust Bracket Bolts | 40 N·m | 30 lb ft
Exhaust Front Pipe-to-Exhaust Manifold Nuts | 40 N·m | 30 lb ft
Exhaust Front Pipe-to-Underbody Shield Nuts | 2.5 N·m | 22 lb in
Exhaust Front/Rear Muffler Shield Nuts | 2.5 N·m | 22 lb in
Exhaust Manifold Heat Shield Bolts | 3 N·m | 27 lb in
Exhaust Rear Muffler-to-Exhaust Front Muffler Nuts | 30 N·m | 22 lb ft
Front Muffler Pipe-to-the 3rd Muffler Nut | 30 N·m | 22 lb ft
Lower Front Exhaust Pipe Mounting Bracket Nut | 30 N·m | 22 lb ft