For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the console cover.
3. Remove the screws and the ashtray trim panel.
4. Disconnect the electrical connectors.
5. Remove the screws and the ashtray housing.
6. Disconnect the cigar lighter electrical connector.
7. Remove the cigar lighter from the cigar lighter housing.
8. Remove the cigar lighter housing from the ashtray housing.

### Installation Procedure

1. Install the cigar lighter housing in the ashtray housing.
2. Install the cigar lighter in the cigar lighter housing.
3. Connect the cigar lighter electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the ashtray housing.

Tighten
Tighten the ashtray housing screws to 2.5 N·m (22 lb in).

5. Connect the electrical connectors.
6. Install the ashtray housing trim panel with the screws.

Tighten
Tighten the ashtray housing screws to 2.5 N·m (22 b in).

7. Install the shift lever trim panel.
8. Connect the negative battery cable.