For 1990-2009 cars

## Front Fog Lamp Replacement 2.5L

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws that secure the fog lamp assembly.
3. Remove the fog lamp assembly.
4. Disconnect the fog lamp assembly electrical connector.
5. Remove the screws and fog lamp access cover.
6. Remove the retaining wire.
7. Remove the bulb from the fog lamp assembly.
8. Disconnect the bulb electrical connector.

### Installation Procedure

1. Connect the bulb electrical connector.
2. Install the bulb from the fog lamp assembly.
3. Install the retaining wire.
4. Install the fog lamp access cover with the screws.
5. Connect the fog lamp assembly electrical connector.
6. Install the fog lamp assembly.
7. Install the fog lamp assembly with the screws.
8. Connect the negative battery cable.

## Front Fog Lamp Replacement 2.0L

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws that secure the fog lamp assembly.
3. Remove the fog lamp assembly.
4. Disconnect the fog lamp assembly electrical connector.
5. Remove the screws and fog lamp access cover.
6. Remove the retaining wire.
7. Remove the bulb from the fog lamp assembly.
8. Disconnect the bulb electrical connector.

### Installation Procedure

1. Connect the bulb electrical connector.
2. Install the bulb from the fog lamp assembly.
3. Install the retaining wire.
4. Install the fog lamp access cover with the screws.
5. Connect the fog lamp assembly electrical connector.
6. Install the fog lamp assembly.
7. Install the fog lamp assembly with the screws.
8. Connect the negative battery cable.