For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the engine cover. Refer to Engine Cover Replacement .
3. Disconnect the EGR vacuum solenoid valve inlet/outlet hoses.
4. Disconnect the EGR vacuum solenoid valve connector.
5. Remove the EGR vacuum solenoid valve.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the EGR vacuum solenoid valve.

Tighten
Tighten the EGR vacuum solenoid valve retaining bolts to 7 N·m (62 lb in).

2. Connect the EGR vacuum solenoid valve connector.
3. Connect the EGR vacuum solenoid valve inlet/outlet hoses.
4. Install the engine cover. Refer to Engine Cover Replacement .
5. Connect the negative battery cable.