For 1990-2009 cars

Checks | Actions
--- | ---
With the steering wheel in the straight-ahead position, remove the key and rotate the steering wheel 120 degrees to the right. | If the steering column does not lock after 120 degree rotation, remove the trim panels around the ignition lock cylinder and lower the steering column. Refer to Ignition Lock Cylinder Replacement .
Check the lock cylinder for damage. | Replace the lock cylinder.
Check the ignition switch for a lack of free movement. | Lubricate the ignition switch.
Check the steering column housing for binding or damage. | Remove the steering shaft and clear the steering column housing. Replace the steering column housing as needed.