For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Mark the position of the hood latch on the radiator support to aid in alignment during installation.
3. Remove the bolts and the hood latch.
4. Disconnect the hood release cable.

### Installation Procedure

1. Connect the hood release cable to the latch.
2. Position the hood latch in the location marked during removal.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the hood latch with the bolts.

Tighten
Tighten the hood latch bolts to 10 N·m (89 lb in).

4. Close the hood.